Date: 02/11/2011 by Nazrul Islam

After Dan’s review on the latest CalLite model, the following modifications are needed:

1. ANNSacFlow.wresl – all model will have C\_yoloBP;
2. JerseyPoint\_output.wresl – needed to remove C\_YoloBP from netDeltaInflow calculation for the purpose of calculating ANN MRDO in both study and corroboration.
3. ExportEstimate1.wresl- to prevent overly aggressive pumping under pumping under negative carriage water quality conditions in June, needed to move export estimate logic based on B2 to cycle 1.