Date: 02/11/2011 by Nazrul Islam

During review, Nancy and Dan made the following modifications:

1. ANNSacFlow.wresl –need to constrain C\_YoloBP\_mif in both the CalLite study and CalLite corroboration;
2. JerseyPoint\_output.wresl – needed to remove C\_YoloBP from netDeltaInflow calculation for the purpose of calculating ANN MRDO in both study and corroboration.
3. ExportEstimate1.wresl- to prevent overly aggressive pumping under pumping under negative carriage water quality conditions in June, needed to move export estimate logic based on B2 to cycle 1.
4. EXP\_constraint.wresl – D\_Banks changed to D\_Banks\_SWP