CalLite Edits: (Dan Easton)

1. CVP\_Delivery\_rule\_curve.wresl
   1. The rulecurve logic in CalLite was inconsistent with the CalSim logic. I looked at previous B2 simulations and the logic in the current CalSim D1641 study is a match. So the CalLite rulecurve logic was updated.
2. FMStandard.wresl
   1. I\_Folsm was not properly indexed in the May-Sep summation AmerFrcstInflow
   2. I\_Folsm is different than I300 + I8 because I300 is upstream of the American River Pump Station and I\_Folsm includes inflow that has already been reduced by ARPS diversions. The 21./5. was added to account for the ARPS diversion since this is likely part of the diversion estimate pulled from the lookup table.